Warning: liberty_arcs_one2one_1.lib line 48, timing port A and related port Y are different sizes.
report_edges -from partial_wide_inv_cell/A[0]
A[0] -> Y[0] combinational
  ^ -> v 1.00:1.00
  v -> ^ 1.00:1.00
report_edges -from partial_wide_inv_cell/A[1]
A[1] -> Y[1] combinational
  ^ -> v 1.00:1.00
  v -> ^ 1.00:1.00
report_edges -from partial_wide_inv_cell/A[2]
A[2] -> Y[2] combinational
  ^ -> v 1.00:1.00
  v -> ^ 1.00:1.00
report_edges -from partial_wide_inv_cell/A[3]
A[3] -> Y[3] combinational
  ^ -> v 1.00:1.00
  v -> ^ 1.00:1.00
report_edges -from partial_wide_inv_cell/A[4]
report_edges -from partial_wide_inv_cell/A[5]
report_edges -from partial_wide_inv_cell/A[6]
report_edges -from partial_wide_inv_cell/A[7]
