Warning: liberty_arcs_one2one_2.lib line 48, timing port A and related port Y are different sizes.
report_edges -to partial_wide_inv_cell/Y[0]
A[0] -> Y[0] combinational
  ^ -> v 1.00:1.00
  v -> ^ 1.00:1.00
report_edges -to partial_wide_inv_cell/Y[1]
A[1] -> Y[1] combinational
  ^ -> v 1.00:1.00
  v -> ^ 1.00:1.00
report_edges -to partial_wide_inv_cell/Y[2]
A[2] -> Y[2] combinational
  ^ -> v 1.00:1.00
  v -> ^ 1.00:1.00
report_edges -to partial_wide_inv_cell/Y[3]
A[3] -> Y[3] combinational
  ^ -> v 1.00:1.00
  v -> ^ 1.00:1.00
report_edges -to partial_wide_inv_cell/Y[4]
report_edges -to partial_wide_inv_cell/Y[5]
report_edges -to partial_wide_inv_cell/Y[6]
report_edges -to partial_wide_inv_cell/Y[7]
