Startpoint: r2 (rising edge-triggered flip-flop clocked by clk)
Endpoint: r3 (rising edge-triggered flip-flop clocked by clk)
Path Group: clk
Path Type: max

  Delay    Time   Description
---------------------------------------------------------
   0.00    0.00   clock clk (rise edge)
   0.00    0.00   clock network delay (ideal)
   0.00    0.00 ^ r2/CK (DFF_X1)
   2.58    2.58 ^ r2/Q (DFF_X1)
   2.58    5.16 ^ u1/Z (BUF_X1)
   2.75    7.91 ^ u2/ZN (AND2_X1)
   0.00    7.92 ^ r3/D (DFF_X1)
           7.92   data arrival time

  10.00   10.00   clock clk (rise edge)
   0.00   10.00   clock network delay (ideal)
   0.00   10.00   clock reconvergence pessimism
          10.00 ^ r3/CK (DFF_X1)
  -0.57    9.43   library setup time
           9.43   data required time
---------------------------------------------------------
           9.43   data required time
          -7.92   data arrival time
---------------------------------------------------------
           1.52   slack (MET)


