Startpoint: in1 (input port clocked by clk)
Endpoint: r1 (rising edge-triggered flip-flop clocked by clk)
Path Group: clk
Path Type: min

  Delay    Time   Description
---------------------------------------------------------
   0.00    0.00   clock clk (rise edge)
   0.00    0.00   clock network delay (ideal)
   0.00    0.00 v input external delay
   0.00    0.00 v in1 (in)
   0.00    0.00 v r1/D (DFF_X1)
           0.00   data arrival time

   0.00    0.00   clock clk (rise edge)
   0.00    0.00   clock network delay (ideal)
   0.00    0.00   clock reconvergence pessimism
           0.00 ^ r1/CK (DFF_X1)
   0.00    0.00   library hold time
           0.00   data required time
---------------------------------------------------------
           0.00   data required time
          -0.00   data arrival time
---------------------------------------------------------
           0.00   slack (VIOLATED)


Startpoint: r2 (rising edge-triggered flip-flop clocked by clk)
Endpoint: r3 (rising edge-triggered flip-flop clocked by clk)
Path Group: clk
Path Type: max

  Delay    Time   Description
---------------------------------------------------------
   0.00    0.00   clock clk (rise edge)
   0.00    0.00   clock network delay (ideal)
   0.00    0.00 ^ r2/CK (DFF_X1)
   0.23    0.23 v r2/Q (DFF_X1)
   0.08    0.31 v u1/Z (BUF_X1)
   0.10    0.41 v u2/ZN (AND2_X1)
   0.00    0.41 v r3/D (DFF_X1)
           0.41   data arrival time

  10.00   10.00   clock clk (rise edge)
   0.00   10.00   clock network delay (ideal)
   0.00   10.00   clock reconvergence pessimism
          10.00 ^ r3/CK (DFF_X1)
  -0.16    9.84   library setup time
           9.84   data required time
---------------------------------------------------------
           9.84   data required time
          -0.41   data arrival time
---------------------------------------------------------
           9.43   slack (MET)


