Find b1/out2: b1/out2
Find b2/out2: b2/out2
Net b2/out2
 Pin capacitance: 0.00
 Wire capacitance: 0.00
 Total capacitance: 0.00
 Number of drivers: 1
 Number of loads: 0
 Number of pins: 1

Driver pins
 b2/u3/Y output (BUFx2_ASAP7_75t_R)

