Using AIG Package in ABC

- Download the latest snapshot of ABC
- Compile the code found in "abc\src\aig\aig", "abc\src\aig\saig", and "abc\src\misc\vec" as a static library.
- Link the library to the project.
- Add #include "saig.h".
- Start the AIG package using Aig_ManStart().
- Assign primary inputs using Aig_ObjCreateCi().
- Assign register outputs using Aig_ObjCreateCi().
(it is important to create all PIs first, before creating register outputs).
- Construct AIG in the topological order using Aig_And(), Aig_Or(), Aig_Not(), etc.
- If constant-0/1 AIG nodes are needed, use Aig_ManConst0() or Aig_ManConst1()
- Create primary outputs using Aig_ObjCreateCo().
- Create register inputs using Aig_ObjCreateCo().
(it is important to create all POs first, before creating register inputs).
- Set the number of registers by calling Aig_ManSetRegNum().
- Remove dangling AIG nodes (produced by structural hashing) using Aig_ManCleanup().
- Call the consistency checking procedure Aig_ManCheck().
- Dump AIG into a file using the new BLIF dumper Saig_ManDumpBlif().
- For each object in the design annotated with the constructed AIG node (pNode), remember its AIG node ID by calling Aig_ObjId( Aig_Regular(pNode) ). To check whether the corresponding AIG node is complemented use Aig_IsComplement(pNode).
- Quit the AIG package using Aig_ManStop().
The above process should not produce memory leaks.



Using GIA Package in ABC

- Add #include "gia.h".
- Start the AIG package using Gia_ManStart( int nObjMax ).
(Parameter 'nNodeMax' should approximately reflect the expected number of objects, including PIs, POs, flop inputs, and flop outputs.  If the number of objects is more, memory will be automatically reallocated.)
- Assign primary inputs using Gia_ManAppendCi().
- Assign flop outputs using Gia_ManAppendCi().
(It is important to create all PIs first, before creating flop outputs).
(Flop control logic, if present, should be elaborated into AND gates.  For example, to represent a flop enable, create the driver of enable signal, which can be a PI or an internal node, and then add logic for <flop_input_new> = MUX( <enable>, <flop_input>, <flop_output> ).  The output of this logic feeds into the flop.
- Construct AIG in the topological order using Gia_ManHashAnd(), Gia_ManHashOr(), Gia_Not(), etc.
- If constant-0/1 AIG nodes are needed, use Gia_ManConst0() or Gia_ManConst1()
- Create primary outputs using Gia_ManAppendCo().
- Create flop inputs using Gia_ManAppendCo().
(it is important to create all POs first, before creating register inputs).
- Set the number of flops by calling Gia_ManSetRegNum().
- Remove dangling AIG nodes (produced by structural hashing) by running Gia_ManCleanup(), which will return a new AIG.  If object mapping is defined for the original AIG, it should be remapped into the new AIG.
- Dump AIG into an AIGER file use Gia_DumpAiger().
- For each object in the design annotated with the constructed AIG node (pNode), remember its AIG node ID by calling Gia_ObjId(pNode).
- Quit the AIG package using Gia_ManStop().
The above process should not produce memory leaks.
