:vpi_module "system";

; Copyright (c) 2001-2008  Stephen Williams (steve@icarus.com)
;
;    This source code is free software; you can redistribute it
;    and/or modify it in source code form under the terms of the GNU
;    General Public License as published by the Free Software
;    Foundation; either version 2 of the License, or (at your option)
;    any later version.
;
;    This program is distributed in the hope that it will be useful,
;    but WITHOUT ANY WARRANTY; without even the implied warranty of
;    MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
;    GNU General Public License for more details.
;
;    You should have received a copy of the GNU General Public License
;    along with this program; if not, write to the Free Software
;    Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA 02111-1307, USA


; This example is similar to the code that the following Verilog program
; would make:
;
;    module main;
;       reg a;
;       wire b = a;
;       initial begin
;          a = 0;
;          #1 $display("a=%b, b=%b", a, b);
;          a = 1;
;          #1 $display("a=%b, b=%b", a, b);
;       end
;    endmodule
;
; This tests that a simple continuous assign of a net from a var works
; properly. This is a very trivial functor propagation that is initiated
; by the %set instruction.

main	.scope module, "main";

V_main.a	.var "a", 0 0;
V_main.b	.net "b", 0 0, V_main.a;

code
	%set/v V_main.a, 0, 1;
	%delay 1, 0;
	%vpi_call 0 0 "$display", "a=%b, b=%b", V_main.a, V_main.b;
	%set/v V_main.a, 1, 1;
	%delay 1, 0;
	%vpi_call 0 0 "$display", "a=%b, b=%b", V_main.a, V_main.b;
	%end;

	.thread	code;
:file_names 2;
    "N/A";
    "<interactive>";
