VERSION 5.8 ;
DIVIDERCHAR "/" ;
BUSBITCHARS "[]" ;
DESIGN comp_invalid_via ;
UNITS DISTANCE MICRONS 1000 ;
DIEAREA ( 0 0 ) ( 10000 2000 ) ;

SPECIALNETS 2 ;
    - VGND ( PIN VGND ) ( * VNB ) ( * VGND ) + USE GROUND
      + ROUTED met1 480 + SHAPE FOLLOWPIN ( 0 1000 ) ( 2000 1000 )
      NEW met1 0 + SHAPE STRIPE ( 2000 1000 ) via1
      + ROUTED met2 480 + SHAPE FOLLOWPIN ( 2000 1000 ) ( 4000 1000 )
      NEW met2 0 + SHAPE STRIPE ( 4000 1000 ) invalid_via ;
END SPECIALNETS
END DESIGN

