//======================================================================================
//======================================================================================
// Filename: JUNCAP200_parlist.include
//======================================================================================
//======================================================================================
//
//  (c) Copyright notice
//
//  Since 2015 until today, PSP has been co-developed by NXP Semiconductors and
//  CEA-Leti. For this part of the model, each claim undivided ownership and copyrights
//  Since 2012 until 2015, PSP has been co-developed by NXP Semiconductors and
//  Delft University of Technology. For this part of the model, each claim undivided
//  ownership and copyrights
//  Until and including 2011, PSP has been co-developed by NXP Semiconductors and
//  Arizona State University. For this part of the model, NXP Semiconductors claims
//  undivided ownership and copyrights.
//
//
//  Version: 200.6.0, April 2019
//
//======================================================================================
//======================================================================================
//
// Further information can be found in the file releasenotesPSP103.txt
//

//  --------------------------------------------------------------------------------------------------------------
//  JUNCAP2 - Reduced parameter list
//  --------------------------------------------------------------------------------------------------------------

`MPRco(IMAX           ,1000.0     ,"A"        ,`IMAX_cliplow     ,inf              ,"Maximum current up to which forward current behaves exponentially")
`MPRco(TRJ            ,21.0       ,"degC"     ,`TRJ_cliplow      ,inf              ,"Reference temperature")
`MPRcc(FREV           ,1.0e3      ,""         ,`FREV_cliplow     ,`FREV_cliphigh   ,"Coefficient for reverse breakdown current limitation")
`IPRcz(IFACTOR        ,1.0        ,""                                              ,"Multiplier for current")
`IPRcz(CFACTOR        ,1.0        ,""                                              ,"Multiplier for depletion capacitance")

// Parameters for source-bulk junction
`ifdef JUNCAP_StandAlone
    `MPRco(CJORBOT        ,1.0e-3     ,"Fm^-2"    ,`CJORBOT_cliplow  ,inf              ,"Zero-bias capacitance per unit-of-area of bottom component")
    `MPRco(CJORSTI        ,1.0e-9     ,"Fm^-1"    ,`CJORSTI_cliplow  ,inf              ,"Zero-bias capacitance per unit-of-length of STI-edge component")
    `MPRco(CJORGAT        ,1.0e-9     ,"Fm^-1"    ,`CJORGAT_cliplow  ,inf              ,"Zero-bias capacitance per unit-of-length of gate-edge component")
    `MPRco(VBIRBOT        ,1.0        ,"V"        ,`VBIR_cliplow     ,inf              ,"Built-in voltage at the reference temperature of bottom component")
    `MPRco(VBIRSTI        ,1.0        ,"V"        ,`VBIR_cliplow     ,inf              ,"Built-in voltage at the reference temperature of STI-edge component")
    `MPRco(VBIRGAT        ,1.0        ,"V"        ,`VBIR_cliplow     ,inf              ,"Built-in voltage at the reference temperature of gate-edge component")
    `MPRcc(PBOT           ,0.5        ,""         ,`P_cliplow        ,`P_cliphigh      ,"Grading coefficient of bottom component")
    `MPRcc(PSTI           ,0.5        ,""         ,`P_cliplow        ,`P_cliphigh      ,"Grading coefficient of STI-edge component")
    `MPRcc(PGAT           ,0.5        ,""         ,`P_cliplow        ,`P_cliphigh      ,"Grading coefficient of gate-edge component")
    `MPRnb(PHIGBOT        ,1.16       ,"V"                                             ,"Zero-temperature bandgap voltage of bottom component")
    `MPRnb(PHIGSTI        ,1.16       ,"V"                                             ,"Zero-temperature bandgap voltage of STI-edge component")
    `MPRnb(PHIGGAT        ,1.16       ,"V"                                             ,"Zero-temperature bandgap voltage of gate-edge component")
    `MPRco(IDSATRBOT      ,1.0e-12    ,"Am^-2"    ,`IDSATR_cliplow   ,inf              ,"Saturation current density at the reference temperature of bottom component")
    `MPRco(IDSATRSTI      ,1.0e-18    ,"Am^-1"    ,`IDSATR_cliplow   ,inf              ,"Saturation current density at the reference temperature of STI-edge component")
    `MPRco(IDSATRGAT      ,1.0e-18    ,"Am^-1"    ,`IDSATR_cliplow   ,inf              ,"Saturation current density at the reference temperature of gate-edge component")
    `MPRco(CSRHBOT        ,1.0e2      ,"Am^-3"    ,`CSRH_cliplow     ,inf              ,"Shockley-Read-Hall prefactor of bottom component")
    `MPRco(CSRHSTI        ,1.0e-4     ,"Am^-2"    ,`CSRH_cliplow     ,inf              ,"Shockley-Read-Hall prefactor of STI-edge component")
    `MPRco(CSRHGAT        ,1.0e-4     ,"Am^-2"    ,`CSRH_cliplow     ,inf              ,"Shockley-Read-Hall prefactor of gate-edge component")
    `MPRco(XJUNSTI        ,1.0e-7     ,"m"        ,`XJUN_cliplow     ,inf              ,"Junction depth of STI-edge component")
    `MPRco(XJUNGAT        ,1.0e-7     ,"m"        ,`XJUN_cliplow     ,inf              ,"Junction depth of gate-edge component")
    `MPRco(CTATBOT        ,1.0e2      ,"Am^-3"    ,`CTAT_cliplow     ,inf              ,"Trap-assisted tunneling prefactor of bottom component")
    `MPRco(CTATSTI        ,1.0e-4     ,"Am^-2"    ,`CTAT_cliplow     ,inf              ,"Trap-assisted tunneling prefactor of STI-edge component")
    `MPRco(CTATGAT        ,1.0e-4     ,"Am^-2"    ,`CTAT_cliplow     ,inf              ,"Trap-assisted tunneling prefactor of gate-edge component")
    `MPRco(MEFFTATBOT     ,0.25       ,""         ,`MEFFTAT_cliplow  ,inf              ,"Effective mass (in units of m0) for trap-assisted tunneling of bottom component")
    `MPRco(MEFFTATSTI     ,0.25       ,""         ,`MEFFTAT_cliplow  ,inf              ,"Effective mass (in units of m0) for trap-assisted tunneling of STI-edge component")
    `MPRco(MEFFTATGAT     ,0.25       ,""         ,`MEFFTAT_cliplow  ,inf              ,"Effective mass (in units of m0) for trap-assisted tunneling of gate-edge component")
    `MPRco(CBBTBOT        ,1.0e-12    ,"AV^-3"    ,`CBBT_cliplow     ,inf              ,"Band-to-band tunneling prefactor of bottom component")
    `MPRco(CBBTSTI        ,1.0e-18    ,"AV^-3m"   ,`CBBT_cliplow     ,inf              ,"Band-to-band tunneling prefactor of STI-edge component")
    `MPRco(CBBTGAT        ,1.0e-18    ,"AV^-3m"   ,`CBBT_cliplow     ,inf              ,"Band-to-band tunneling prefactor of gate-edge component")
    `MPRnb(FBBTRBOT       ,1.0e9      ,"Vm^-1"                                         ,"Normalization field at the reference temperature for band-to-band tunneling of bottom component")
    `MPRnb(FBBTRSTI       ,1.0e9      ,"Vm^-1"                                         ,"Normalization field at the reference temperature for band-to-band tunneling of STI-edge component")
    `MPRnb(FBBTRGAT       ,1.0e9      ,"Vm^-1"                                         ,"Normalization field at the reference temperature for band-to-band tunneling of gate-edge component")
    `MPRnb(STFBBTBOT      ,-1.0e-3    ,"K^-1"                                          ,"Temperature scaling parameter for band-to-band tunneling of bottom component")
    `MPRnb(STFBBTSTI      ,-1.0e-3    ,"K^-1"                                          ,"Temperature scaling parameter for band-to-band tunneling of STI-edge component")
    `MPRnb(STFBBTGAT      ,-1.0e-3    ,"K^-1"                                          ,"Temperature scaling parameter for band-to-band tunneling of gate-edge component")
    `MPRco(VBRBOT         ,10.0       ,"V"        ,`VBR_cliplow      ,inf              ,"Breakdown voltage of bottom component")
    `MPRco(VBRSTI         ,10.0       ,"V"        ,`VBR_cliplow      ,inf              ,"Breakdown voltage of STI-edge component")
    `MPRco(VBRGAT         ,10.0       ,"V"        ,`VBR_cliplow      ,inf              ,"Breakdown voltage of gate-edge component")
    `MPRco(PBRBOT         ,4.0        ,"V"        ,`PBR_cliplow      ,inf              ,"Breakdown onset tuning parameter of bottom component")
    `MPRco(PBRSTI         ,4.0        ,"V"        ,`PBR_cliplow      ,inf              ,"Breakdown onset tuning parameter of STI-edge component")
    `MPRco(PBRGAT         ,4.0        ,"V"        ,`PBR_cliplow      ,inf              ,"Breakdown onset tuning parameter of gate-edge component")
`else // JUNCAP_StandAlone
    `MPRco(CJORBOT        ,1.0e-3     ,"Fm^-2"    ,`CJORBOT_cliplow  ,inf              ,"Zero-bias capacitance per unit-of-area of bottom component for source-bulk junction")
    `MPRco(CJORSTI        ,1.0e-9     ,"Fm^-1"    ,`CJORSTI_cliplow  ,inf              ,"Zero-bias capacitance per unit-of-length of STI-edge component for source-bulk junction")
    `MPRco(CJORGAT        ,1.0e-9     ,"Fm^-1"    ,`CJORGAT_cliplow  ,inf              ,"Zero-bias capacitance per unit-of-length of gate-edge component for source-bulk junction")
    `MPRco(VBIRBOT        ,1.0        ,"V"        ,`VBIR_cliplow     ,inf              ,"Built-in voltage at the reference temperature of bottom component for source-bulk junction")
    `MPRco(VBIRSTI        ,1.0        ,"V"        ,`VBIR_cliplow     ,inf              ,"Built-in voltage at the reference temperature of STI-edge component for source-bulk junction")
    `MPRco(VBIRGAT        ,1.0        ,"V"        ,`VBIR_cliplow     ,inf              ,"Built-in voltage at the reference temperature of gate-edge component for source-bulk junction")
    `MPRcc(PBOT           ,0.5        ,""         ,`P_cliplow        ,`P_cliphigh      ,"Grading coefficient of bottom component for source-bulk junction")
    `MPRcc(PSTI           ,0.5        ,""         ,`P_cliplow        ,`P_cliphigh      ,"Grading coefficient of STI-edge component for source-bulk junction")
    `MPRcc(PGAT           ,0.5        ,""         ,`P_cliplow        ,`P_cliphigh      ,"Grading coefficient of gate-edge component for source-bulk junction")
    `MPRnb(PHIGBOT        ,1.16       ,"V"                                             ,"Zero-temperature bandgap voltage of bottom component for source-bulk junction")
    `MPRnb(PHIGSTI        ,1.16       ,"V"                                             ,"Zero-temperature bandgap voltage of STI-edge component for source-bulk junction")
    `MPRnb(PHIGGAT        ,1.16       ,"V"                                             ,"Zero-temperature bandgap voltage of gate-edge component for source-bulk junction")
    `MPRco(IDSATRBOT      ,1.0e-12    ,"Am^-2"    ,`IDSATR_cliplow   ,inf              ,"Saturation current density at the reference temperature of bottom component for source-bulk junction")
    `MPRco(IDSATRSTI      ,1.0e-18    ,"Am^-1"    ,`IDSATR_cliplow   ,inf              ,"Saturation current density at the reference temperature of STI-edge component for source-bulk junction")
    `MPRco(IDSATRGAT      ,1.0e-18    ,"Am^-1"    ,`IDSATR_cliplow   ,inf              ,"Saturation current density at the reference temperature of gate-edge component for source-bulk junction")
    `MPRco(CSRHBOT        ,1.0e2      ,"Am^-3"    ,`CSRH_cliplow     ,inf              ,"Shockley-Read-Hall prefactor of bottom component for source-bulk junction")
    `MPRco(CSRHSTI        ,1.0e-4     ,"Am^-2"    ,`CSRH_cliplow     ,inf              ,"Shockley-Read-Hall prefactor of STI-edge component for source-bulk junction")
    `MPRco(CSRHGAT        ,1.0e-4     ,"Am^-2"    ,`CSRH_cliplow     ,inf              ,"Shockley-Read-Hall prefactor of gate-edge component for source-bulk junction")
    `MPRco(XJUNSTI        ,1.0e-7     ,"m"        ,`XJUN_cliplow     ,inf              ,"Junction depth of STI-edge component for source-bulk junction")
    `MPRco(XJUNGAT        ,1.0e-7     ,"m"        ,`XJUN_cliplow     ,inf              ,"Junction depth of gate-edge component for source-bulk junction")
    `MPRco(CTATBOT        ,1.0e2      ,"Am^-3"    ,`CTAT_cliplow     ,inf              ,"Trap-assisted tunneling prefactor of bottom component for source-bulk junction")
    `MPRco(CTATSTI        ,1.0e-4     ,"Am^-2"    ,`CTAT_cliplow     ,inf              ,"Trap-assisted tunneling prefactor of STI-edge component for source-bulk junction")
    `MPRco(CTATGAT        ,1.0e-4     ,"Am^-2"    ,`CTAT_cliplow     ,inf              ,"Trap-assisted tunneling prefactor of gate-edge component for source-bulk junction")
    `MPRco(MEFFTATBOT     ,0.25       ,""         ,`MEFFTAT_cliplow  ,inf              ,"Effective mass (in units of m0) for trap-assisted tunneling of bottom component for source-bulk junction")
    `MPRco(MEFFTATSTI     ,0.25       ,""         ,`MEFFTAT_cliplow  ,inf              ,"Effective mass (in units of m0) for trap-assisted tunneling of STI-edge component for source-bulk junction")
    `MPRco(MEFFTATGAT     ,0.25       ,""         ,`MEFFTAT_cliplow  ,inf              ,"Effective mass (in units of m0) for trap-assisted tunneling of gate-edge component for source-bulk junction")
    `MPRco(CBBTBOT        ,1.0e-12    ,"AV^-3"    ,`CBBT_cliplow     ,inf              ,"Band-to-band tunneling prefactor of bottom component for source-bulk junction")
    `MPRco(CBBTSTI        ,1.0e-18    ,"AV^-3m"   ,`CBBT_cliplow     ,inf              ,"Band-to-band tunneling prefactor of STI-edge component for source-bulk junction")
    `MPRco(CBBTGAT        ,1.0e-18    ,"AV^-3m"   ,`CBBT_cliplow     ,inf              ,"Band-to-band tunneling prefactor of gate-edge component for source-bulk junction")
    `MPRnb(FBBTRBOT       ,1.0e9      ,"Vm^-1"                                         ,"Normalization field at the reference temperature for band-to-band tunneling of bottom component for source-bulk junction")
    `MPRnb(FBBTRSTI       ,1.0e9      ,"Vm^-1"                                         ,"Normalization field at the reference temperature for band-to-band tunneling of STI-edge component for source-bulk junction")
    `MPRnb(FBBTRGAT       ,1.0e9      ,"Vm^-1"                                         ,"Normalization field at the reference temperature for band-to-band tunneling of gate-edge component for source-bulk junction")
    `MPRnb(STFBBTBOT      ,-1.0e-3    ,"K^-1"                                          ,"Temperature scaling parameter for band-to-band tunneling of bottom component for source-bulk junction")
    `MPRnb(STFBBTSTI      ,-1.0e-3    ,"K^-1"                                          ,"Temperature scaling parameter for band-to-band tunneling of STI-edge component for source-bulk junction")
    `MPRnb(STFBBTGAT      ,-1.0e-3    ,"K^-1"                                          ,"Temperature scaling parameter for band-to-band tunneling of gate-edge component for source-bulk junction")
    `MPRco(VBRBOT         ,10.0       ,"V"        ,`VBR_cliplow      ,inf              ,"Breakdown voltage of bottom component for source-bulk junction")
    `MPRco(VBRSTI         ,10.0       ,"V"        ,`VBR_cliplow      ,inf              ,"Breakdown voltage of STI-edge component for source-bulk junction")
    `MPRco(VBRGAT         ,10.0       ,"V"        ,`VBR_cliplow      ,inf              ,"Breakdown voltage of gate-edge component for source-bulk junction")
    `MPRco(PBRBOT         ,4.0        ,"V"        ,`PBR_cliplow      ,inf              ,"Breakdown onset tuning parameter of bottom component for source-bulk junction")
    `MPRco(PBRSTI         ,4.0        ,"V"        ,`PBR_cliplow      ,inf              ,"Breakdown onset tuning parameter of STI-edge component for source-bulk junction")
    `MPRco(PBRGAT         ,4.0        ,"V"        ,`PBR_cliplow      ,inf              ,"Breakdown onset tuning parameter of gate-edge component for source-bulk junction")
`endif // JUNCAP_StandAlone

// Parameters for drain-bulk junction
`ifdef JUNCAP_StandAlone
    // do nothing
`else // JUNCAP_StandAlone
    `MPRco(CJORBOTD       ,1.0e-3     ,"Fm^-2"    ,`CJORBOT_cliplow  ,inf              ,"Zero-bias capacitance per unit-of-area of bottom component for drain-bulk junction")
    `MPRco(CJORSTID       ,1.0e-9     ,"Fm^-1"    ,`CJORSTI_cliplow  ,inf              ,"Zero-bias capacitance per unit-of-length of STI-edge component for drain-bulk junction")
    `MPRco(CJORGATD       ,1.0e-9     ,"Fm^-1"    ,`CJORGAT_cliplow  ,inf              ,"Zero-bias capacitance per unit-of-length of gate-edge component for drain-bulk junction")
    `MPRco(VBIRBOTD       ,1.0        ,"V"        ,`VBIR_cliplow     ,inf              ,"Built-in voltage at the reference temperature of bottom component for drain-bulk junction")
    `MPRco(VBIRSTID       ,1.0        ,"V"        ,`VBIR_cliplow     ,inf              ,"Built-in voltage at the reference temperature of STI-edge component for drain-bulk junction")
    `MPRco(VBIRGATD       ,1.0        ,"V"        ,`VBIR_cliplow     ,inf              ,"Built-in voltage at the reference temperature of gate-edge component for drain-bulk junction")
    `MPRcc(PBOTD          ,0.5        ,""         ,`P_cliplow        ,`P_cliphigh      ,"Grading coefficient of bottom component for drain-bulk junction")
    `MPRcc(PSTID          ,0.5        ,""         ,`P_cliplow        ,`P_cliphigh      ,"Grading coefficient of STI-edge component for drain-bulk junction")
    `MPRcc(PGATD          ,0.5        ,""         ,`P_cliplow        ,`P_cliphigh      ,"Grading coefficient of gate-edge component for drain-bulk junction")
    `MPRnb(PHIGBOTD       ,1.16       ,"V"                                             ,"Zero-temperature bandgap voltage of bottom component for drain-bulk junction")
    `MPRnb(PHIGSTID       ,1.16       ,"V"                                             ,"Zero-temperature bandgap voltage of STI-edge component for drain-bulk junction")
    `MPRnb(PHIGGATD       ,1.16       ,"V"                                             ,"Zero-temperature bandgap voltage of gate-edge component for drain-bulk junction")
    `MPRco(IDSATRBOTD     ,1.0e-12    ,"Am^-2"    ,`IDSATR_cliplow   ,inf              ,"Saturation current density at the reference temperature of bottom component for drain-bulk junction")
    `MPRco(IDSATRSTID     ,1.0e-18    ,"Am^-1"    ,`IDSATR_cliplow   ,inf              ,"Saturation current density at the reference temperature of STI-edge component for drain-bulk junction")
    `MPRco(IDSATRGATD     ,1.0e-18    ,"Am^-1"    ,`IDSATR_cliplow   ,inf              ,"Saturation current density at the reference temperature of gate-edge component for drain-bulk junction")
    `MPRco(CSRHBOTD       ,1.0e2      ,"Am^-3"    ,`CSRH_cliplow     ,inf              ,"Shockley-Read-Hall prefactor of bottom component for drain-bulk junction")
    `MPRco(CSRHSTID       ,1.0e-4     ,"Am^-2"    ,`CSRH_cliplow     ,inf              ,"Shockley-Read-Hall prefactor of STI-edge component for drain-bulk junction")
    `MPRco(CSRHGATD       ,1.0e-4     ,"Am^-2"    ,`CSRH_cliplow     ,inf              ,"Shockley-Read-Hall prefactor of gate-edge component for drain-bulk junction")
    `MPRco(XJUNSTID       ,1.0e-7     ,"m"        ,`XJUN_cliplow     ,inf              ,"Junction depth of STI-edge component for drain-bulk junction")
    `MPRco(XJUNGATD       ,1.0e-7     ,"m"        ,`XJUN_cliplow     ,inf              ,"Junction depth of gate-edge component for drain-bulk junction")
    `MPRco(CTATBOTD       ,1.0e2      ,"Am^-3"    ,`CTAT_cliplow     ,inf              ,"Trap-assisted tunneling prefactor of bottom component for drain-bulk junction")
    `MPRco(CTATSTID       ,1.0e-4     ,"Am^-2"    ,`CTAT_cliplow     ,inf              ,"Trap-assisted tunneling prefactor of STI-edge component for drain-bulk junction")
    `MPRco(CTATGATD       ,1.0e-4     ,"Am^-2"    ,`CTAT_cliplow     ,inf              ,"Trap-assisted tunneling prefactor of gate-edge component for drain-bulk junction")
    `MPRco(MEFFTATBOTD    ,0.25       ,""         ,`MEFFTAT_cliplow  ,inf              ,"Effective mass (in units of m0) for trap-assisted tunneling of bottom component for drain-bulk junction")
    `MPRco(MEFFTATSTID    ,0.25       ,""         ,`MEFFTAT_cliplow  ,inf              ,"Effective mass (in units of m0) for trap-assisted tunneling of STI-edge component for drain-bulk junction")
    `MPRco(MEFFTATGATD    ,0.25       ,""         ,`MEFFTAT_cliplow  ,inf              ,"Effective mass (in units of m0) for trap-assisted tunneling of gate-edge component for drain-bulk junction")
    `MPRco(CBBTBOTD       ,1.0e-12    ,"AV^-3"    ,`CBBT_cliplow     ,inf              ,"Band-to-band tunneling prefactor of bottom component for drain-bulk junction")
    `MPRco(CBBTSTID       ,1.0e-18    ,"AV^-3m"   ,`CBBT_cliplow     ,inf              ,"Band-to-band tunneling prefactor of STI-edge component for drain-bulk junction")
    `MPRco(CBBTGATD       ,1.0e-18    ,"AV^-3m"   ,`CBBT_cliplow     ,inf              ,"Band-to-band tunneling prefactor of gate-edge component for drain-bulk junction")
    `MPRnb(FBBTRBOTD      ,1.0e9      ,"Vm^-1"                                         ,"Normalization field at the reference temperature for band-to-band tunneling of bottom component for drain-bulk junction")
    `MPRnb(FBBTRSTID      ,1.0e9      ,"Vm^-1"                                         ,"Normalization field at the reference temperature for band-to-band tunneling of STI-edge component for drain-bulk junction")
    `MPRnb(FBBTRGATD      ,1.0e9      ,"Vm^-1"                                         ,"Normalization field at the reference temperature for band-to-band tunneling of gate-edge component for drain-bulk junction")
    `MPRnb(STFBBTBOTD     ,-1.0e-3    ,"K^-1"                                          ,"Temperature scaling parameter for band-to-band tunneling of bottom component for drain-bulk junction")
    `MPRnb(STFBBTSTID     ,-1.0e-3    ,"K^-1"                                          ,"Temperature scaling parameter for band-to-band tunneling of STI-edge component for drain-bulk junction")
    `MPRnb(STFBBTGATD     ,-1.0e-3    ,"K^-1"                                          ,"Temperature scaling parameter for band-to-band tunneling of gate-edge component for drain-bulk junction")
    `MPRco(VBRBOTD        ,10.0       ,"V"        ,`VBR_cliplow      ,inf              ,"Breakdown voltage of bottom component for drain-bulk junction")
    `MPRco(VBRSTID        ,10.0       ,"V"        ,`VBR_cliplow      ,inf              ,"Breakdown voltage of STI-edge component for drain-bulk junction")
    `MPRco(VBRGATD        ,10.0       ,"V"        ,`VBR_cliplow      ,inf              ,"Breakdown voltage of gate-edge component for drain-bulk junction")
    `MPRco(PBRBOTD        ,4.0        ,"V"        ,`PBR_cliplow      ,inf              ,"Breakdown onset tuning parameter of bottom component for drain-bulk junction")
    `MPRco(PBRSTID        ,4.0        ,"V"        ,`PBR_cliplow      ,inf              ,"Breakdown onset tuning parameter of STI-edge component for drain-bulk junction")
    `MPRco(PBRGATD        ,4.0        ,"V"        ,`PBR_cliplow      ,inf              ,"Breakdown onset tuning parameter of gate-edge component for drain-bulk junction")
`endif // JUNCAP_StandAlone

// JUNCAP2-express parameters
`MPRcc(SWJUNEXP       ,0.0        ,""         ,0.0               ,1.0              ,"Flag for JUNCAP-express; 0=full model, 1=express model")
`ifdef JUNCAP_StandAlone
    `MPRco(VJUNREF        ,2.5        ,"V"        ,`VJUNREF_cliplow  ,inf              ,"Typical maximum junction voltage; usually about 2*VSUP")
    `MPRco(FJUNQ          ,0.03       ,""         ,`FJUNQ_cliplow    ,inf              ,"Fraction below which junction capacitance components are considered negligible")
`else // JUNCAP_StandAlone
    `MPRco(VJUNREF        ,2.5        ,"V"        ,`VJUNREF_cliplow  ,inf              ,"Typical maximum source-bulk junction voltage; usually about 2*VSUP")
    `MPRco(FJUNQ          ,0.03       ,""         ,`FJUNQ_cliplow    ,inf              ,"Fraction below which source-bulk junction capacitance components are considered negligible")
    `MPRco(VJUNREFD       ,2.5        ,"V"        ,`VJUNREF_cliplow  ,inf              ,"Typical maximum drain-bulk junction voltage; usually about 2*VSUP")
    `MPRco(FJUNQD         ,0.03       ,""         ,`FJUNQ_cliplow    ,inf              ,"Fraction below which drain-bulk junction capacitance components are considered negligible")
`endif // JUNCAP_StandAlone
