# Loosely based on
# ./utils/bits2fasm.py --db-root database/artix7 --canonical utils/test_data/ff_int/design.bits

# FF as LDCE
CLBLM_L_X10Y102.SLICEM_X0.AFFMUX.AX
CLBLM_L_X10Y102.SLICEM_X0.AFF.ZINI
CLBLM_L_X10Y102.SLICEM_X0.AFF.ZRST
CLBLM_L_X10Y102.SLICEM_X0.CEUSEDMUX
CLBLM_L_X10Y102.SLICEM_X0.SRUSEDMUX
# Unused bits explicitly set to 0
CLBLM_L_X10Y102.SLICEM_X0.FFSYNC = 0
CLBLM_L_X10Y102.SLICEM_X0.LATCH = 0

# Note: a number of pseudo pips here
# Omitted
INT_L_X10Y102.BYP_ALT0.EE2END0
INT_L_X10Y102.BYP_ALT1.EL1END1
INT_L_X10Y102.CLK_L1.GCLK_L_B11_WEST
INT_L_X10Y102.CTRL_L1.ER1END2
INT_L_X10Y102.FAN_ALT7.BYP_BOUNCE0
INT_L_X10Y102.WW2BEG0.LOGIC_OUTS_L4

HCLK_L_X31Y130.ENABLE_BUFFER.HCLK_CK_BUFHCLK8
HCLK_L_X31Y130.HCLK_LEAF_CLK_B_BOTL5.HCLK_CK_BUFHCLK8

