v {xschem version=3.4.4 file_version=1.2
*
* This file is part of XSCHEM,
* a schematic capture and Spice/Vhdl/Verilog netlisting tool for circuit
* simulation.
* Copyright (C) 1998-2023 Stefan Frederik Schippers
*
* This program is free software; you can redistribute it and/or modify
* it under the terms of the GNU General Public License as published by
* the Free Software Foundation; either version 2 of the License, or
* (at your option) any later version.
*
* This program is distributed in the hope that it will be useful,
* but WITHOUT ANY WARRANTY; without even the implied warranty of
* MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
* GNU General Public License for more details.
*
* You should have received a copy of the GNU General Public License
* along with this program; if not, write to the Free Software
* Foundation, Inc., 51 Franklin Street, Fifth Floor, Boston, MA 02110-1301 USA
}
G {}
K {type=probe
vhdl_ignore=true
spice_ignore=false
verilog_ignore=true
tedax_ignore=true
template="name=r1
devicename=M1
devicemodel=nfet_01v8
deviceparam=gm"}
V {}
S {}
E {}
A 15 0 0 1.875 90 360 {fill=true}
T {tcleval([ngspice::get_node \\@m.[set path]x@devicename\\.msky130_fd_pr__@devicemodel\\\\[@deviceparam\\\\]])
} 4.375 -8.59375 0 0 0.2 0.2 {vcenter=true layer=15}
T {@deviceparam\\=} 4.375 -26.09375 0 0 0.2 0.2 {vcenter=true layer=15}
T {@devicemodel} 4.375 -41.09375 0 0 0.2 0.2 {vcenter=true layer=15}
T {@devicename} 4.375 -56.09375 0 0 0.2 0.2 {vcenter=true layer=15}
