v {xschem version=3.4.4 file_version=1.2
*
* This file is part of XSCHEM,
* a schematic capture and Spice/Vhdl/Verilog netlisting tool for circuit
* simulation.
* Copyright (C) 1998-2023 Stefan Frederik Schippers
*
* This program is free software; you can redistribute it and/or modify
* it under the terms of the GNU General Public License as published by
* the Free Software Foundation; either version 2 of the License, or
* (at your option) any later version.
*
* This program is distributed in the hope that it will be useful,
* but WITHOUT ANY WARRANTY; without even the implied warranty of
* MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
* GNU General Public License for more details.
*
* You should have received a copy of the GNU General Public License
* along with this program; if not, write to the Free Software
* Foundation, Inc., 51 Franklin Street, Fifth Floor, Boston, MA 02110-1301 USA
}
G {type=npn
format="* @name @pinlist  @model"
tedax_format="footprint @name @footprint
value @name @value
device @name @device
@comptag"
template="name=C1
model=usb-minib
device="UX60SC-MB-5ST(80)"
footprint=hirose-UX60SC
"
}
V {}
S {}
E {}
L 4 -60 -80 -60 80 {}
L 4 -60 -80 60 -80 {}
L 4 60 -80 60 80 {}
L 4 -60 80 -30 80 {}
L 4 -5 -40 -5 40 {}
L 4 -15 -40 -5 -40 {}
L 4 -30 -25 -15 -40 {}
L 4 -40 -25 -40 25 {}
L 4 -30 25 -15 40 {}
L 4 -15 40 -5 40 {}
L 4 -40 25 -30 25 {}
L 4 -40 -25 -30 -25 {}
L 4 -50 -80 -50 80 {}
L 4 -20 90 -20 120 {}
L 4 60 -60 80 -60 {}
L 4 60 -30 80 -30 {}
L 4 60 0 80 0 {}
L 4 60 30 80 30 {}
L 4 60 60 80 60 {}
L 4 20 90 20 120 {}
L 4 30 80 60 80 {}
L 4 -10 80 10 80 {}
B 5 77.5 -62.5 82.5 -57.5 {name=V5V dir=inout pinnumber=1}
B 5 77.5 -32.5 82.5 -27.5 {name=DM dir=inout pinnumber=2}
B 5 77.5 -2.5 82.5 2.5 {name=DP dir=inout pinnumber=3}
B 5 77.5 27.5 82.5 32.5 {name=ID dir=inout pinnumber=4}
B 5 77.5 57.5 82.5 62.5 {name=GND dir=inout pinnumber=5}
B 5 -22.5 117.5 -17.5 122.5 {name=G1 dir=inout pinnumber=6}
B 5 17.5 117.5 22.5 122.5 {name=G2 dir=inout pinnumber=7}
A 4 -20 80 10 180 360 {}
A 4 20 80 10 180 360 {}
T {@model} -40 -75 0 0 0.2 0.2 {}
T {@name} 20 -95 0 0 0.2 0.2 {}
T {V5V} 55 -65 0 1 0.2 0.2 {}
T {DM} 55 -35 0 1 0.2 0.2 {}
T {DP} 55 -5 0 1 0.2 0.2 {}
T {ID} 55 25 0 1 0.2 0.2 {}
T {GND} 55 55 0 1 0.2 0.2 {}
T {G1} -15 55 0 1 0.2 0.2 {}
T {@#0:pinnumber} 63.75 -76.25 0 0 0.2 0.2 {layer=13}
T {@#1:pinnumber} 63.75 -46.25 0 0 0.2 0.2 {layer=13}
T {@#2:pinnumber} 63.75 -16.25 0 0 0.2 0.2 {layer=13}
T {@#3:pinnumber} 63.75 13.75 0 0 0.2 0.2 {layer=13}
T {@#4:pinnumber} 63.75 43.75 0 0 0.2 0.2 {layer=13}
T {@#6:pinnumber} 23.75 93.75 0 0 0.2 0.2 {layer=13}
T {G2} 25 55 0 1 0.2 0.2 {}
T {@#5:pinnumber} -23.75 93.75 0 1 0.2 0.2 {layer=13}
