v {xschem version=3.4.4 file_version=1.2
*
* This file is part of XSCHEM,
* a schematic capture and Spice/Vhdl/Verilog netlisting tool for circuit
* simulation.
* Copyright (C) 1998-2023 Stefan Frederik Schippers
*
* This program is free software; you can redistribute it and/or modify
* it under the terms of the GNU General Public License as published by
* the Free Software Foundation; either version 2 of the License, or
* (at your option) any later version.
*
* This program is distributed in the hope that it will be useful,
* but WITHOUT ANY WARRANTY; without even the implied warranty of
* MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
* GNU General Public License for more details.
*
* You should have received a copy of the GNU General Public License
* along with this program; if not, write to the Free Software
* Foundation, Inc., 51 Franklin Street, Fifth Floor, Boston, MA 02110-1301 USA
}
G {type=regulator
format="@spiceprefix@name @pinlist @symname"

tedax_format="footprint @name @footprint
device @name @symname"

template="name=U1 device=MAX882 footprint=SO8"}
V {}
S {}
E {}
L 4 -200 -40 -160 -40 {}
L 4 -200 0 -160 0 {}
L 4 -200 40 -160 40 {}
L 7 160 -40 200 -40 {}
L 7 160 40 200 40 {}
L 9 -120 100 -120 140 {}
L 9 80 100 80 140 {}
L 9 120 100 120 140 {}
B 5 -202.5 -42.5 -197.5 -37.5 {name=STBY_ dir=in pinnumber=7}
B 5 -202.5 -2.5 -197.5 2.5 {name=IN dir=in pinnumber=5}
B 5 -202.5 37.5 -197.5 42.5 {name=LBI dir=in pinnumber=8}
B 5 197.5 -42.5 202.5 -37.5 {name=LBO dir=out pinnumber=1}
B 5 197.5 37.5 202.5 42.5 {name=OUT dir=out pinnumber=4}
B 5 -122.5 137.5 -117.5 142.5 {name=SET dir=inout pinnumber=2}
B 5 77.5 137.5 82.5 142.5 {name=GND dir=inout pinnumber=3}
B 5 117.5 137.5 122.5 142.5 {name=GND dir=inout pinnumber=6}
P 4 5 -160 -100 160 -100 160 100 -160 100 -160 -100 {}
T {STBY_} -149 -49.6 0 0 0.4 0.4 {}
T {7} -172 -56 0 1 0.25 0.25 {layer=13}
T {IN} -149 -9.6 0 0 0.4 0.4 {}
T {5} -172 -16 0 1 0.25 0.25 {layer=13}
T {LBI} -149 30.4 0 0 0.4 0.4 {}
T {8} -172 24 0 1 0.25 0.25 {layer=13}
T {LBO} 149 -49.6 0 1 0.4 0.4 {}
T {1} 172 -56 0 0 0.25 0.25 {layer=13}
T {OUT} 149 30.4 0 1 0.4 0.4 {}
T {4} 172 24 0 0 0.25 0.25 {layer=13}
T {SET} -141 89 2 1 0.4 0.4 {}
T {2} -136 112 3 1 0.25 0.25 {layer=13}
T {3} 64 112 3 1 0.25 0.25 {layer=13}
T {GND} 79 89 2 1 0.4 0.4 {}
T {6} 104 112 3 1 0.25 0.25 {layer=13}
T {@device} -63 -18 0 0 0.6 0.6 {}
T {@name} 160 -143 0 1 0.6 0.6 {}
