### TODO: Not running equivalence checking because BRAM models does not exists
###       currently. Checking instance counts instead.
# Memory bits <= 18K; Data width <= 36; Address width <= 14: -> RBRAM2
read_verilog ../common/blockram.v
chparam -set ADDRESS_WIDTH 12 -set DATA_WIDTH 1 sync_ram_sdp
setattr -set ram_style "block" sync_ram_sdp
synth_analogdevices -top sync_ram_sdp -noiopad
cd sync_ram_sdp
select -assert-count 1 t:RBRAM2

design -reset
read_verilog ../common/blockram.v
chparam -set ADDRESS_WIDTH 8 -set DATA_WIDTH 18 sync_ram_sdp
setattr -set ram_style "block" sync_ram_sdp
synth_analogdevices -top sync_ram_sdp -noiopad
cd sync_ram_sdp
select -assert-count 1 t:RBRAM2

design -reset
read_verilog ../common/blockram.v
chparam -set ADDRESS_WIDTH 14 -set DATA_WIDTH 1 sync_ram_sdp
setattr -set ram_style "block" sync_ram_sdp
synth_analogdevices -top sync_ram_sdp -noiopad
cd sync_ram_sdp
select -assert-count 1 t:RBRAM2

design -reset
read_verilog ../common/blockram.v
chparam -set ADDRESS_WIDTH 9 -set DATA_WIDTH 36 sync_ram_sdp
synth_analogdevices -top sync_ram_sdp -noiopad
cd sync_ram_sdp
select -assert-count 1 t:RBRAM2

# Anything memory bits < 1024 -> LUTRAM
design -reset
read_verilog ../common/blockram.v
chparam -set ADDRESS_WIDTH 8 -set DATA_WIDTH 2 sync_ram_sdp
synth_analogdevices -top sync_ram_sdp -noiopad
cd sync_ram_sdp
select -assert-count 0 t:RBRAM2
select -assert-count 8 t:RAMD64X1
select -assert-count 2 t:FFRE

# More than 18K bits, data width <= 36 (TDP), and address width from 10 to 15b (non-cascaded) -> RAMB36E1
design -reset
read_verilog ../common/blockram.v
chparam -set ADDRESS_WIDTH 10 -set DATA_WIDTH 36 sync_ram_sdp
synth_analogdevices -top sync_ram_sdp -noiopad
cd sync_ram_sdp
select -assert-count 1 t:RBRAM2


### With parameters

design -reset
read_verilog ../common/blockram.v
hierarchy -top sync_ram_sdp -chparam ADDRESS_WIDTH 12 -chparam DATA_WIDTH 1 
setattr -set ram_style "block" m:memory
synth_analogdevices -top sync_ram_sdp -noiopad
cd sync_ram_sdp
select -assert-count 1 t:RBRAM2

design -reset
read_verilog ../common/blockram.v
hierarchy -top sync_ram_sdp -chparam ADDRESS_WIDTH 12 -chparam DATA_WIDTH 1 
setattr -set logic_block 1 m:memory
synth_analogdevices -top sync_ram_sdp -noiopad
cd sync_ram_sdp
select -assert-count 0 t:RBRAM2

design -reset
read_verilog ../common/blockram.v
hierarchy -top sync_ram_sdp -chparam ADDRESS_WIDTH 8 -chparam DATA_WIDTH 1
setattr -set ram_style "block" m:memory
synth_analogdevices -top sync_ram_sdp -noiopad
cd sync_ram_sdp
select -assert-count 1 t:RBRAM2
