# ISC License
# 
# Copyright (C) 2024 Microchip Technology Inc. and its subsidiaries
# 
# Permission to use, copy, modify, and/or distribute this software for any
# purpose with or without fee is hereby granted, provided that the above
# copyright notice and this permission notice appear in all copies.
# 
# THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
# WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
# MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
# ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
# WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
# ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF
# OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.

read_verilog <<EOT
module uram_sr(clk, wr, raddr, din, waddr, dout);
	input clk;
	input [11:0] din;
	input wr;
	input [5:0] waddr, raddr;
	output [11:0] dout;
	reg [5:0] raddr_reg;
	reg [11:0] mem [0:63];
	assign dout = mem[raddr_reg];
	integer i;
	initial begin
		for (i = 0; i < 64; i = i + 1) begin
			mem[i] = 12'hfff;
		end
	end

	always@(posedge clk) begin
		raddr_reg <= raddr; 
		if(wr)
			mem[waddr]<= din;
	end
endmodule
EOT

synth_microchip -top uram_sr -family polarfire -noiopad

select -assert-count 1 t:RAM64x12
select -assert-none t:RAM64x12 %% t:* %D
