# ISC License
# 
# Copyright (C) 2024 Microchip Technology Inc. and its subsidiaries
# 
# Permission to use, copy, modify, and/or distribute this software for any
# purpose with or without fee is hereby granted, provided that the above
# copyright notice and this permission notice appear in all copies.
# 
# THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
# WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
# MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
# ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
# WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
# ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF
# OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.

read_verilog <<EOT
module ram_SDP(data,waddr,we,clk,q);
parameter d_width = 32;
parameter addr_width = 8;
parameter mem_depth = 256;
input [d_width-1:0] data;
input [addr_width-1:0] waddr;
input we, clk;
output reg [d_width-1:0] q;

reg [d_width-1:0] mem [mem_depth-1:0];

always @(posedge clk) begin
	if (we) begin 
		mem[waddr] <= data;
	end else begin
		q <= mem[waddr];
	end
end
endmodule
EOT
synth_microchip -top ram_SDP -family polarfire -noiopad
select -assert-count 1 t:RAM1K20
select -assert-count 1 t:CFG1
select -assert-none t:RAM1K20 t:CFG1 %% t:* %D

# very similar to ram_SDP.v, except read enable is always active
design -reset
read_verilog ../common/blockram.v
hierarchy -top sync_ram_sdp
chparam -set DATA_WIDTH 32 -set ADDRESS_WIDTH 8
synth_microchip -top sync_ram_sdp -family polarfire -noiopad
select -assert-count 1 t:RAM1K20
select -assert-none t:RAM1K20 %% t:* %D