# Check wires driven by constants are kept
read_verilog <<EOT
module top(output wire [7:0] y);
assign y = 27;
endmodule
EOT

equiv_opt -assert bufnorm
design -load postopt
select -assert-count 1 t:$buf
select -assert-count 1 w:y %ci t:$buf %i
