Startpoint: in1 (input port clocked by clk)
Endpoint: r1 (rising edge-triggered flip-flop clocked by clk)
Path Group: clk
Path Type: min
Corner: ss

  Delay    Time   Description
---------------------------------------------------------
   0.00    0.00   clock clk (rise edge)
   0.00    0.00   clock network delay (ideal)
   0.00    0.00 ^ input external delay
   0.00    0.00 ^ in1 (in)
   0.00    0.00 ^ r1/D (DFF_X1)
           0.00   data arrival time

   0.00    0.00   clock clk (rise edge)
   0.00    0.00   clock network delay (ideal)
   0.00    0.00   clock reconvergence pessimism
           0.00 ^ r1/CK (DFF_X1)
   0.01    0.01   library hold time
           0.01   data required time
---------------------------------------------------------
           0.01   data required time
          -0.00   data arrival time
---------------------------------------------------------
          -0.01   slack (VIOLATED)


Startpoint: r2 (rising edge-triggered flip-flop clocked by clk)
Endpoint: r3 (rising edge-triggered flip-flop clocked by clk)
Path Group: clk
Path Type: max
Corner: ss

  Delay    Time   Description
---------------------------------------------------------
   0.00    0.00   clock clk (rise edge)
   0.00    0.00   clock network delay (ideal)
   0.00    0.00 ^ r2/CK (DFF_X1)
   0.26    0.26 v r2/Q (DFF_X1)
   0.09    0.35 v u1/Z (BUF_X1)
   0.11    0.46 v u2/ZN (AND2_X1)
   0.00    0.46 v r3/D (DFF_X1)
           0.46   data arrival time

  10.00   10.00   clock clk (rise edge)
   0.00   10.00   clock network delay (ideal)
   0.00   10.00   clock reconvergence pessimism
          10.00 ^ r3/CK (DFF_X1)
  -0.16    9.84   library setup time
           9.84   data required time
---------------------------------------------------------
           9.84   data required time
          -0.46   data arrival time
---------------------------------------------------------
           9.38   slack (MET)


Startpoint: r2 (rising edge-triggered flip-flop clocked by clk)
Endpoint: r3 (rising edge-triggered flip-flop clocked by clk)
Path Group: clk
Path Type: max
Corner: tt

  Delay    Time   Description
---------------------------------------------------------
   0.00    0.00   clock clk (rise edge)
   0.00    0.00   clock network delay (ideal)
   0.00    0.00 ^ r2/CK (DFF_X1)
   0.09    0.09 v r2/Q (DFF_X1)
   0.03    0.11 v u1/Z (BUF_X1)
   0.03    0.14 v u2/ZN (AND2_X1)
   0.00    0.14 v r3/D (DFF_X1)
           0.14   data arrival time

  10.00   10.00   clock clk (rise edge)
   0.00   10.00   clock network delay (ideal)
   0.00   10.00   clock reconvergence pessimism
          10.00 ^ r3/CK (DFF_X1)
  -0.04    9.96   library setup time
           9.96   data required time
---------------------------------------------------------
           9.96   data required time
          -0.14   data arrival time
---------------------------------------------------------
           9.82   slack (MET)


