
//
// CMC test specification for bsimsoi (version 4.4)
//

//
// Simulator specific information
// These arguments are added to the model card
// specification to invoke the desired model in
// different simulators (which can have different
// names or levels for the same model) and to switch
// between nType and pType polarities.
// It is assumed that there are no polarity specific
// parameters.
//

`ifdef spice
nTypeSelectionArguments nmos level=10
pTypeSelectionArguments pmos level=10
`endif 
`ifdef ngspice
nTypeSelectionArguments nmos level=10
pTypeSelectionArguments pmos level=10
`endif
`ifdef hspice
nTypeSelectionArguments nmos level=70 version=4.4
pTypeSelectionArguments pmos level=70 version=4.4
`endif

//
// General test-independent information
//

keyLetter                   m
pins                        d g s b
linearScale                 w l ps pd
areaScale                   as ad
temperature                 27 -50 150
checkPolarity               no
symmetricPins               d s
scaleParameters             m

//
// Specific tests
//

test                        dcSweep01
biases                      V(s)=0 V(b)=0
biasList                    V(g)=-1.6,0.4,1.6
biasSweep                   V(d)=0.1,1.6,0.1
outputs                     I(d)
instanceParameters          w=0.2e-6 l=0.04e-6
modelParameters             parameters/nmosParameters
modelParameters             soimod=0 mobmod=1

test                        dcSweep02
biases                      V(s)=0 V(b)=0
biasList                    V(g)=-1.6,0.4,1.6
biasSweep                   V(d)=0.1,1.6,0.1
outputs                     I(d)
instanceParameters          w=0.2e-6 l=0.04e-6
modelParameters             parameters/nmosParameters
modelParameters             soimod=1 mobmod=2

test                        dcSweep03
biases                      V(s)=0 V(b)=0
biasList                    V(g)=-1.6,0.4,1.6
biasSweep                   V(d)=0.1,1.6,0.1
outputs                     I(d)
instanceParameters          w=0.2e-6 l=0.04e-6
modelParameters             parameters/nmosParameters
modelParameters             soimod=3 mobmod=3

test                        acVd01
temperature                 27 150
biases                      V(s)=0 V(b)=0 V(g)=1.2
biasSweep                   V(d)=0.1,1.2,0.1
outputs                     G(d,g) G(d,d) C(g,s) C(g,d)
instanceParameters          w=0.2e-6 l=0.04e-6
modelParameters             parameters/nmosParameters
modelParameters             soimod=0 capmod=2

test                        acVd02
temperature                 27 150
biases                      V(s)=0 V(b)=0 V(g)=1.2
biasSweep                   V(d)=0.1,1.2,0.1
outputs                     G(d,g) G(d,d) C(g,s) C(g,d)
instanceParameters          w=0.2e-6 l=0.04e-6
modelParameters             parameters/nmosParameters
modelParameters             soimod=1 capmod=3

test                        acFreq01
temperature                 27
biases                      V(s)=0 V(b)=0 V(d)=1.2 V(g)=1.2
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          w=0.2e-6 l=0.04e-6
modelParameters             parameters/nmosParameters
modelParameters             soimod=0 capmod=2

test                        acFreq02
temperature                 27
biases                      V(s)=0 V(b)=0 V(d)=1.2 V(g)=1.2
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          w=0.2e-6 l=0.04e-6
modelParameters             parameters/nmosParameters
modelParameters             soimod=3 capmod=3

test                        noise01
temperature                 27
biases                      V(s)=0 V(b)=0 V(d)=1.0
biasList                    V(g)=0.6,0.8,1.0
freq                        dec 10 1e3 1e8
outputs                     N(d)
instanceParameters          w=0.2e-6 l=0.04e-6
modelParameters             parameters/nmosParameters
modelParameters             soimod=0 fnoimod=0 tnoimod=0

test                        noise02
temperature                 27
biases                      V(s)=0 V(b)=0 V(d)=1.0
biasList                    V(g)=0.6,0.8,1.0
freq                        dec 10 1e3 1e8
outputs                     N(d)
instanceParameters          w=0.2e-6 l=0.04e-6
modelParameters             parameters/nmosParameters
modelParameters             soimod=1 fnoimod=1 tnoimod=1

test                        noise03
temperature                 27
biases                      V(s)=0 V(b)=0 V(d)=1.0
biasList                    V(g)=0.6,0.8,1.0
freq                        dec 10 1e3 1e8
outputs                     N(d)
instanceParameters          w=0.2e-6 l=0.04e-6
modelParameters             parameters/nmosParameters
modelParameters             soimod=3 fnoimod=1 tnoimod=2
