/*.......1.........2.........3.........4.........5.........6.........7.........8
================================================================================
Copyright 2018
Holger Vogt
All Rights Reserved

AUTHORS

     2 October 2018     Holger Vogt


SUMMARY

    This file contains the interface specification file for the
    analog simple diode code model.

===============================================================================*/

NAME_TABLE:


C_Function_Name:       cm_sidiode
Spice_Model_Name:      sidiode
Description:           "simple diode"


PORT_TABLE:


Port_Name:             ds
Description:           "diode port"
Direction:             inout
Default_Type:          gd
Allowed_Types:         [gd]
Vector:                 no
Vector_Bounds:          -
Null_Allowed:          no


PARAMETER_TABLE:


Parameter_Name:     ron                      roff
Description:        "resistance on-state"    "resistance off-state"
Data_Type:          real                     real
Default_Value:      1                        1
Limits:             [1e-6  - ]               [1e-12 -]
Vector:              no                       no
Vector_Bounds:       -                        -
Null_Allowed:       no                       no


PARAMETER_TABLE:

Parameter_Name:    vfwd                      vrev
Description:       "forward voltage"         "reverse breakdown voltage"
Data_Type:     	   real                      real
Default_Value:     0.                        1e30
Limits:            [0. -]                    [0. -]
Vector:             no                        no
Vector_Bounds:      -                         -
Null_Allowed:      yes                       yes



PARAMETER_TABLE:

Parameter_Name:     ilimit                   revilimit
Description:        "limit of on-current"    "limit of breakdown current"
Data_Type:          real                     real
Default_Value:      1e30                     1e30
Limits:             [1e-15 -]                [1e-15 -]
Vector:              no                       no
Vector_Bounds:       -                        -
Null_Allowed:       yes                      yes


PARAMETER_TABLE:

Parameter_Name:    epsilon                   revepsilon
Description:       "width quadrat. r 1"      "width quadratic region 2"
Data_Type:     	   real                      real
Default_Value:     0.                        0.
Limits:            [0. -]                    [0. -]
Vector:             no                        no
Vector_Bounds:      -                         -
Null_Allowed:      yes                       yes



PARAMETER_TABLE:

Parameter_Name:     rrev
Description:        "resistance in breakdown"
Data_Type:          real
Default_Value:      0.
Limits:             -
Vector:              no
Vector_Bounds:       -
Null_Allowed:       yes



STATIC_VAR_TABLE:

Static_Var_Name:    locdata
Data_Type:          pointer
Description:        "table with constants"
