/* ===========================================================================
FILE    ifspec.ifs

MEMBER OF process XSPICE

Copyright 1991
Georgia Tech Research Corporation
Atlanta, Georgia 30332
All Rights Reserved

PROJECT A-8503

AUTHORS

    9/12/91  Bill Kuhn

MODIFICATIONS

    <date> <person name> <nature of modifications>

SUMMARY

    This file contains the definition of a capacitor code model
    with voltage type initial conditions.

INTERFACES

    None.

REFERENCED FILES

    None.

NON-STANDARD FEATURES

    None.

=========================================================================== */

NAME_TABLE:

Spice_Model_Name:      capacitor
C_Function_Name:       cm_capacitor
Description:           "Capacitor with voltage initial condition"


PORT_TABLE:

Port_Name:             cap
Description:           "capacitor terminals"
Direction:             inout
Default_Type:          hd
Allowed_Types:         [hd]
Vector:                 no
Vector_Bounds:          -
Null_Allowed:          no


PARAMETER_TABLE:

Parameter_Name:        c                ic
Description:           "capacitance"    "voltage initial condition"
Data_Type:             real             real
Default_Value:         -                0.0
Limits:                -                -
Vector:                 no               no
Vector_Bounds:          -                -
Null_Allowed:          no               no



