
//
// Test specification for HiSIM (version 2.7.0)
//

//
// Simulator specific information
// These arguments are added to the model card
// specification to invoke the desired model in
// different simulators (which can have different
// names or levels for the same model) and to switch
// between nType and pType polarities.
// It is assumed that there are no polarity specific
// parameters.
//

`ifdef spice
nTypeSelectionArguments nmos level=61 version=270
pTypeSelectionArguments pmos level=61 version=270
`endif
`ifdef ngspice
nTypeSelectionArguments nmos level=68 version=270
pTypeSelectionArguments pmos level=68 version=270
`endif
`ifdef hspice
nTypeSelectionArguments nmos level=68 version=2.7.0
pTypeSelectionArguments pmos level=68 version=2.7.0
`endif

//
// General test-independent information
//

keyLetter                   m
pins                        d g s b 
linearScale                 w l ps pd
areaScale                   as ad 
temperature                 27 -50 150
symmetricPins               d s
scaleParameters             m


//
// Specific tests
//

test                        1_dcSweep_CORSRD=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             CORSRD=0 GDLD=0.001

test                        2_dcSweep_CORSRD=-1_GDLD
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=-1.0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9 
instanceParameters	    NRD=0.1 NRS=0.01 
modelParameters             CORSRD=-1 RSH=1 GDLD=0.0001

test                        3_dcSweep_CORSRD=-1_PT
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0.5
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9 
instanceParameters	    NRD=0.01 NRS=0.1 AD=1e-8 AS=1e-8 PD=1e-3 PS=1e-3
modelParameters             CORSRD=-1 RSH=10 PT4P=0.1

test                        4_dcSweep_NSUBPFAC
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             NSUBPL=0.1 NSUBPFAC=0.6 

test                        5_dcSweep_NSUBPDLT
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             NSUBPL=0.1 NSUBPFAC=0.8 NSUBPDLT=0.001

test                        6_dcSweep_COISUB=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(b)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COISUB=0 SUB1=1 SVGS=1 SVDS=1 SUB1L=0.1 SUB2L=0.1 SLG=1 SVBS=1

test                        7_dcSweep_COISUB=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d) I(b)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COISUB=1 SUB1=1 SVGS=1 SVDS=1 SUB1L=0.1 SUB2L=0.1 SLG=1 SVBS=1

test                        8_dcSweep_COIIGS=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(g)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COIIGS=0 

test                        9_dcSweep_COIIGS=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(g) 
instanceParameters          W=10e-6 L=100e-9
modelParameters             COIIGS=1 

test                        10_dcSweep_COGIDL=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d) I(b)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COGIDL=1 GIDL6=-1.0 GIDL7=1.05

test                        11_dcSweep_COGIDL=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d) I(b)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COGIDL=1 GIDL6=-1.0 

test                        12_dcSweep_COGIDL=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COGIDL=1 GIDL7=1.05

test                        13_dcSweep_COISTI=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COISTI=0 WSTI=0.1E-4
instanceParameters          SA=1e-6  SB=2e-6 SD=1e-6 NF=5
modelParameters             NSUBPSTI1=2e-6 NSUBPSTI2=1e-6 NSUBPSTI3=1.5

test                        14_dcSweep_COISTI=1_NSUBC
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COISTI=1 WSTI=0.1E-4
instanceParameters          SA=1e-6 SB=2e-6 SD=1e-6 NF=5
modelParameters             NSUBCSTI1=2e-6 NSUBCSTI2=1e-6 NSUBCSTI3=1.4

test                        15_dcSweep_COISTI=1_NSUBP
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COISTI=1 WSTI=0.1E-4
instanceParameters          SA=1e-6 SB=2e-6 SD=1e-6 NF=2
modelParameters             NSUBPSTI1=2e-6 NSUBPSTI2=1e-6 NSUBPSTI3=1.5

test                        16_dcSweep_WPE
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             WEB=-1200 WEC=-1200 NSUBCWPE=1E-16 NSUBPWPE=1E16 NPEXTWPE=1E16 
instanceParameters	    SCA=4.244122e-01 SCB=2.561023e-09 SCC=3.215142e-18

test                        19_dcSweep_CORG=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9 NGCON=0.1
modelParameters             CORG=0 RSHG=10

test                        20_dcSweep_CORG=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9 NGCON=0.1
modelParameters             CORG=1 RSHG=10

test                        21_dcSweep_CORBNET=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d) I(b)
instanceParameters          W=10e-6 L=100e-9
modelParameters             CORBNET=0

test                        22_dcSweep_CORBNET=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d) I(b)
instanceParameters          W=10e-6 L=100e-9
modelParameters             CORBNET=1

test                        23_dcSweep_CODFM=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9  NSUBCDFM=1E17
modelParameters             CODFM=0 

test                        24_dcSweep_CODFM=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9  NSUBCDFM=1E17
modelParameters             CODFM=1 

test                        25_dcSweep_VFBCL
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0
biasList                    V(g)=0.4,0.6,0.8,1.0,1.2,1.5,1.8
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     I(d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             VFBCL=0.8 VFBCLP=1.2

test                        35_acVd_CORSRD=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(g)=1.2
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     G(d,g) G(d,d) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             CORSRD=0 GDLD=0.001

test                        36_acVd_CORSRD=-1_GDLD
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=-1.0 V(g)=1.2
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     G(d,g) G(d,d) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
instanceParameters	    NRD=1 NRS=0.1
modelParameters             CORSRD=-1 RSH=10 GDLD=0.001

test                        37_acVd_CORSRD=-1_PT
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0.5 V(g)=1.2
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     G(d,g) G(d,d) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
instanceParameters	    NRD=0.1 NRS=1 AD=1e-8 AS=1e-8 PD=1e-3 PS=1e-3
modelParameters             CORSRD=-1 RSH=100 PT4P=0.1

test                        38_acVd_WPE
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0.5 V(g)=1.2
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     G(d,g) G(d,d) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             WEB=-1200 WEC=-1200 NSUBCWPE=1E-16 NSUBPWPE=2E16 NPEXTWPE=3E16 
instanceParameters	    SCA=4.25e-01 SCB=2.56e-09 SCC=3.2e-18

test                        39_acVd_VFBCL
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0.5 V(g)=1.2
biasSweep                   V(d)=0.2,1.800000000001,0.1
outputs                     G(d,g) G(d,d) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=500e-9
modelParameters             VFBCL=0.8 VFBCLP=1.2


test                        45_acFreq_COOVLP=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COOVLP=1

test                        46_acFreq_COISUB=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COISUB=0  SUB1=1 SVGS=1 SVDS=1 SUB1L=0.1 SUB2L=0.1 SLG=1 SVBS=1

test                        47_acFreq_COISUB=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COISUB=1  SUB1=1 SVGS=1 SVDS=1 SUB1L=0.1 SUB2L=0.1 SLG=1 SVBS=1

test                        48_acFreq_COIIGS=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COIIGS=0 

test                        49_acFreq_COIIGS=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COIIGS=1 

test                        50_acFreq_COGIDL=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COGIDL=0 GIDL6=-1.0 GIDL7=1.05

test                        51_acFreq_COGIDL=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COGIDL=1 GIDL6=-1.0 GIDL7=1.05

test                        52_acFreq_COSTI=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COISTI=0

test                        53_acFreq_COSTI=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COISTI=1

test                        54_acFreq_COADOV=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COADOV=0

test                        55_acFreq_COADOV=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COADOV=1

test                        56_acFreq_CONQS=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             CONQS=0

test                        57_acFreq_CONQS=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             CONQS=1

test                        58_acFreq_CORG=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9 NGCON=0.1
modelParameters             CORG=0 RSHG=10 

test                        59_acFreq_CORG=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9 NGCON=0.1
modelParameters             CORG=1 RSHG=10

test                        60_acFreq_CORBNET=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             CORBNET=0

test                        61_acFreq_CORBNET=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             CORBNET=1

test                        62_acFreq_COFLICK=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COFLICK=0

test                        63_acFreq_COFLICK=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COFLICK=1

test                        64_acFreq_COTHRML=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COTHRML=0

test                        65_acFreq_COTHRML=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COTHRML=1

test                        66_acFreq_COIGN=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COIGN=0

test                        67_acFreq_COIGN=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             COIGN=1

test                        68_acFreq_WPE
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9
modelParameters             WEB=-1200 WEC=-1200 NSUBCWPE=1E-16 NSUBPWPE=1E16 NPEXTWPE=1E16 
instanceParameters	    SCA=4.25e-01 SCB=2.56e-09 SCC=3.2e-18

test                        69_acFreq_CODFM=0
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9  NSUBCDFM=1E17
modelParameters             CODFM=0 

test                        70_acFreq_CODFM=1
temperature                 -55 27 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.5 V(g)=1.5
freq                        dec 10 1e3 1e8
outputs                     C(g,g) C(g,s) C(g,d)
instanceParameters          W=10e-6 L=100e-9  NSUBCDFM=1E17
modelParameters             CODFM=1 

test                        75_noise_COIGN=1_T27
temperature                 27 
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.0
biasList                    V(g)=0.5,1.0
freq                        dec 10 1e3 1e11
outputs                     N(g)
instanceParameters          W=10e-6 L=100e-9 
modelParameters             COIIGS=0 COTHRML=1 COIGN=1 

test                        76_noise_COIGN=1_T-55
temperature                 -55 
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.0
biasList                    V(g)=0.5,1.0
freq                        dec 10 1e3 1e11
outputs                     N(g)
instanceParameters          W=10e-6 L=100e-9 
modelParameters             COIIGS=0 COTHRML=1 COIGN=1 

test                        77_noise_COIGN=1_T150
temperature                 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.0
biasList                    V(g)=0.5,1.0
freq                        dec 10 1e3 1e11
outputs                     N(g)
instanceParameters          W=10e-6 L=100e-9 
modelParameters             COIIGS=0 COTHRML=1 COIGN=1 

test                        78_noise_COIGN=0_T27
temperature                 27 
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.0
biasList                    V(g)=0.5,1.0
freq                        dec 10 1e3 1e11
outputs                     N(g)
instanceParameters          W=10e-6 L=100e-9 
modelParameters             COIIGS=0 COTHRML=1 COIGN=0 COFLICK=1 FALPH=1.0 

test                        79_noise_COIGN=0_T-55
temperature                 -55 
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.0
biasList                    V(g)=0.5,1.0
freq                        dec 10 1e3 1e11
outputs                     N(g)
instanceParameters          W=10e-6 L=100e-9 
modelParameters             COIIGS=0 COTHRML=1 COIGN=0 COFLICK=1 FALPH=1.0 

test                        80_noise_COIGN=0_T150
temperature                 150
modelParameters             parameters/nmosParameters
biases                      V(s)=0 V(b)=0 V(d)=1.0
biasList                    V(g)=0.5,1.0
freq                        dec 10 1e3 1e11
outputs                     N(g)
instanceParameters          W=10e-6 L=100e-9 
modelParameters             COIIGS=0 COTHRML=1 COIGN=0 COFLICK=1 FALPH=1.0 

