/*.......1.........2.........3.........4.........5.........6.........7.........8
================================================================================

-------------------------------------------------------------------------
 Copyright 2005
 Intrinsity, Inc. Austin, TX 78738
 All Rights Reserved
 3 - Clause BSD license
 (see COPYING or https://opensource.org/licenses/BSD-3-Clause)
-------------------------------------------------------------------------

AUTHORS                      

     20 Oct 2005     Phil Barker

SUMMARY

    This file contains the interface specification file for the 
    analog multi-input gate pwl code model.

===============================================================================*/

NAME_TABLE:

C_Function_Name:       cm_multi_input_pwl
Spice_Model_Name:      multi_input_pwl
Description:           "multi_input_pwl block"


PORT_TABLE:

Port_Name:             in                 out
Description:           "input array"      "output"
Direction:             in                 out
Default_Type:          vd                 vd
Allowed_Types:         [vd,id]            [vd,id]
Vector:                yes                no
Vector_Bounds:         [2 -]              -
Null_Allowed:          no                 no


PARAMETER_TABLE:

Parameter_Name:        x                  y               model
Description:           "x array"          "y array"       "model type"
Data_Type:             real               real            string
Default_Value:         0.0                0.0             "and"
Limits:                -                  -               -
Vector:                yes                yes             no
Vector_Bounds:         [2 -]              [2 -]           -
Null_Allowed:          no                 no              yes
