v {xschem version=3.4.4 file_version=1.2
*
* This file is part of XSCHEM,
* a schematic capture and Spice/Vhdl/Verilog netlisting tool for circuit
* simulation.
* Copyright (C) 1998-2023 Stefan Frederik Schippers
*
* This program is free software; you can redistribute it and/or modify
* it under the terms of the GNU General Public License as published by
* the Free Software Foundation; either version 2 of the License, or
* (at your option) any later version.
*
* This program is distributed in the hope that it will be useful,
* but WITHOUT ANY WARRANTY; without even the implied warranty of
* MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
* GNU General Public License for more details.
*
* You should have received a copy of the GNU General Public License
* along with this program; if not, write to the Free Software
* Foundation, Inc., 51 Franklin Street, Fifth Floor, Boston, MA 02110-1301 USA
}
G {}
K {type=subcircuit
format="@name @pinlist @symname OFFSET=@OFFSET AMPLITUDE=@AMPLITUDE GAIN=@GAIN ROUT=@ROUT COUT=@COUT"
template="name=x1 OFFSET=0 AMPLITUDE=5 GAIN=100 ROUT=1000 COUT=1p"
}
V {}
S {}
E {}
L 4 -40 -50 -40 50 {}
L 4 -60 -30 -40 -30 {}
L 4 40 0 60 0 {}
L 4 -60 30 -40 30 {}
L 4 -40 -50 40 0 {}
L 4 -40 50 40 0 {}
B 5 -62.5 -32.5 -57.5 -27.5 {name=PLUS dir=in }
B 5 57.5 -2.5 62.5 2.5 {name=OUT dir=out }
B 5 -62.5 27.5 -57.5 32.5 {name=MINUS dir=in }
T {@symname} -32 44 0 0 0.3 0.3 {}
T {@name} -20 -48.25 0 0 0.2 0.2 {}
T {PLUS} -38.75 -30.25 0 0 0.2 0.2 {}
T {OUT} 28.75 -5.25 0 1 0.2 0.2 {}
T {MINUS} -38.75 18.5 0 0 0.2 0.2 {}
T {GAIN=@GAIN
ROUT=@ROUT
COUT=@COUT} 28 -46 0 0 0.2 0.2 {}
T {OFFSET=@OFFSET} 8.75 32.5 0 0 0.2 0.2 {}
T {AMPLITUDE=@AMPLITUDE} 8.75 21.25 0 0 0.2 0.2 {}
