v {xschem version=3.4.4 file_version=1.2
*
* This file is part of XSCHEM,
* a schematic capture and Spice/Vhdl/Verilog netlisting tool for circuit
* simulation.
* Copyright (C) 1998-2024 Stefan Frederik Schippers
*
* This program is free software; you can redistribute it and/or modify
* it under the terms of the GNU General Public License as published by
* the Free Software Foundation; either version 2 of the License, or
* (at your option) any later version.
*
* This program is distributed in the hope that it will be useful,
* but WITHOUT ANY WARRANTY; without even the implied warranty of
* MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
* GNU General Public License for more details.
*
* You should have received a copy of the GNU General Public License
* along with this program; if not, write to the Free Software
* Foundation, Inc., 51 Franklin Street, Fifth Floor, Boston, MA 02110-1301 USA
}
K {}
G {}
V {}
S {}
E {}
T {USB connector} 5270 -5150 2 1 0.833333 0.833333 {}
T {gTAG - console IO} 6430 -4110 2 1 0.666667 0.666667 {}
T {5} 6440 -4030 2 1 0.333333 0.333333 {}
T {3} 6300 -4030 2 1 0.333333 0.333333 {}
T {gTAG-consio.sch} 6300 -4060 2 1 0.333333 0.333333 {}
T {Stefan Petersen (spe@stacken.kth.se)} 6680 -4030 2 1 0.333333 0.333333 {}
T {$Revision$} 6680 -4060 2 1 0.333333 0.333333 {}






C {title-A2.sym} 4660 -4020 0 0 {}
C {out-1.sym} 5710 -4840 0 1 {name=usb_io+
lab=usb_io+
}
C {out-1.sym} 5710 -4920 0 1 {name=usb_io-
lab=usb_io-
}
C {gnd-1.sym} 5790 -5060 0 0 {}
C {connector4-1.sym} 5610 -5090 0 0 {name=CONN2
footprint=conn_usb
}
C {out-1.sym} 5940 -5190 0 0 {name=usb_power
lab=usb_power
}
C {sn75240pw.sym} 5990 -4810 0 0 {name=U40
}
C {gnd-1.sym} 5960 -4800 0 0 {}
C {gnd-1.sym} 6190 -4800 0 0 {}
C {copyleft.sym} 4690 -4040 0 0 {}

N 5780 -5140 5870 -5140 {}
N 5870 -5140 5870 -4850 {}
N 5780 -5170 5900 -5170 {}
N 5780 -5200 5940 -5200 {}
N 5780 -5110 5800 -5110 {}
N 5800 -5110 5800 -5090 {}
N 5970 -4960 5990 -4960 {}
N 5970 -4960 5970 -4830 {}
N 5970 -4890 5990 -4890 {}
N 6200 -4930 6200 -4830 {}
N 6180 -4930 6200 -4930 {}
N 6180 -4850 6200 -4850 {}
N 5900 -5170 5900 -4930 {}
N 5870 -4850 5990 -4850 {}
N 5900 -4930 5990 -4930 {}
N 5710 -4930 5900 -4930 {}
N 5710 -4850 5870 -4850 {}

