read_verilog ../common/mux.v
design -save read

hierarchy -top mux2
proc
equiv_opt -assert -map +/ecp5/cells_sim.v synth_ecp5 # equivalency check
design -load postopt # load the post-opt design (otherwise equiv_opt loads the pre-opt design)
cd mux2 # Constrain all select calls below inside the top module
select -assert-count 1 t:LUT4
select -assert-none t:LUT4 %% t:* %D

design -load read
hierarchy -top mux4
proc
equiv_opt -assert -map +/ecp5/cells_sim.v synth_ecp5 # equivalency check
design -load postopt # load the post-opt design (otherwise equiv_opt loads the pre-opt design)
cd mux4 # Constrain all select calls below inside the top module
select -assert-max 1 t:L6MUX21
select -assert-max 4 t:LUT4
select -assert-max 2 t:PFUMX

select -assert-none t:LUT4 t:L6MUX21 t:PFUMX %% t:* %D

design -load read
hierarchy -top mux8
proc
equiv_opt -assert -map +/ecp5/cells_sim.v synth_ecp5 # equivalency check
design -load postopt # load the post-opt design (otherwise equiv_opt loads the pre-opt design)
cd mux8 # Constrain all select calls below inside the top module
select -assert-max 1 t:L6MUX21
select -assert-max 8 t:LUT4
select -assert-max 3 t:PFUMX

select -assert-none t:LUT4 t:L6MUX21 t:PFUMX %% t:* %D

design -load read
hierarchy -top mux16
proc
equiv_opt -assert -map +/ecp5/cells_sim.v synth_ecp5 # equivalency check
design -load postopt # load the post-opt design (otherwise equiv_opt loads the pre-opt design)
cd mux16 # Constrain all select calls below inside the top module
select -assert-max 12 t:L6MUX21
select -assert-max 34 t:LUT4
select -assert-max 17 t:PFUMX

select -assert-none t:LUT4 t:L6MUX21 t:PFUMX %% t:* %D
