read_verilog ../common/mux.v
design -save read

hierarchy -top mux2
proc
equiv_opt -assert -map +/gowin/cells_sim.v synth_gowin # equivalency check
design -load postopt # load the post-opt design (otherwise equiv_opt loads the pre-opt design)
cd mux2 # Constrain all select calls below inside the top module
select -assert-count 1 t:LUT3
select -assert-count 3 t:IBUF
select -assert-count 1 t:OBUF

select -assert-none t:LUT3 t:IBUF t:OBUF %% t:* %D

design -load read
hierarchy -top mux4
proc
equiv_opt -assert -map +/gowin/cells_sim.v synth_gowin # equivalency check
design -load postopt # load the post-opt design (otherwise equiv_opt loads the pre-opt design)
cd mux4 # Constrain all select calls below inside the top module
select -assert-count 4 t:LUT*
select -assert-count 2 t:MUX2_LUT5
select -assert-count 1 t:MUX2_LUT6
select -assert-count 6 t:IBUF
select -assert-count 1 t:OBUF

select -assert-none t:LUT* t:MUX2_LUT6 t:MUX2_LUT5 t:IBUF t:OBUF %% t:* %D

design -load read
hierarchy -top mux8
proc
equiv_opt -assert -map +/gowin/cells_sim.v synth_gowin # equivalency check
design -load postopt # load the post-opt design (otherwise equiv_opt loads the pre-opt design)
cd mux8 # Constrain all select calls below inside the top module
select -assert-count 1 t:LUT1
select -assert-count 10 t:LUT3
select -assert-count 1 t:LUT4
select -assert-count 5 t:MUX2_LUT5
select -assert-count 2 t:MUX2_LUT6
select -assert-count 1 t:MUX2_LUT7
select -assert-count 11 t:IBUF
select -assert-count 1 t:OBUF
select -assert-count 1 t:GND

select -assert-none t:LUT* t:MUX2_LUT7 t:MUX2_LUT6 t:MUX2_LUT5 t:IBUF t:OBUF t:GND %% t:* %D

design -load read
hierarchy -top mux16
proc
equiv_opt -assert -map +/gowin/cells_sim.v synth_gowin # equivalency check
design -load postopt # load the post-opt design (otherwise equiv_opt loads the pre-opt design)
cd mux16 # Constrain all select calls below inside the top module
select -assert-count 20 t:IBUF
select -assert-count 1 t:OBUF

select -assert-none t:GND t:VCC t:LUT* t:MUX2_LUT6 t:MUX2_LUT5 t:MUX2_LUT6 t:MUX2_LUT7 t:MUX2_LUT8 t:IBUF t:OBUF %% t:* %D
