# ISC License
# 
# Copyright (C) 2024 Microchip Technology Inc. and its subsidiaries
# 
# Permission to use, copy, modify, and/or distribute this software for any
# purpose with or without fee is hereby granted, provided that the above
# copyright notice and this permission notice appear in all copies.
# 
# THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
# WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
# MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
# ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
# WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
# ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF
# OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.

# regular unsigned multiply
read_verilog ../common/mul.v
chparam -set X_WIDTH 8 -set Y_WIDTH 8 -set A_WIDTH 16
hierarchy -top top
proc
synth_microchip -family polarfire -noiopad
cd top # Constrain all select calls below inside the top module
select -assert-count 1 t:MACC_PA
select -assert-none t:MACC_PA %% t:* %D

# regular signed multiply
design -reset
read_verilog <<EOT
module signed_mult(
	input signed [17:0] in_A,
	input signed [17:0] in_B,
	output signed [35:0] out_Y
);
assign out_Y = in_A * in_B;
endmodule
EOT
synth_microchip -top signed_mult -family polarfire -noiopad
select -assert-count 1 t:MACC_PA
select -assert-none t:MACC_PA %% t:* %D

# wide multiply
design -reset
read_verilog ../common/mul.v
chparam -set X_WIDTH 30 -set Y_WIDTH 16 -set A_WIDTH 46
hierarchy -top top
proc
synth_microchip -family polarfire -noiopad
cd top # Constrain all select calls below inside the top module
select -assert-count 2 t:MACC_PA
select -assert-none t:MACC_PA %% t:* %D
